**Requirement Specification for   
Combi Module (Oxygen/Fixed Suction)**

1. **Requirements**

**1.1. Description of the requirement**

DALO wants to acquire 50 combi modules (oxygen/fixed suction) for the new armored ambulances of the Danish Defence.

The combi modules will be wall mounted in the ambulances. DALO notes that it is imperative that the offered combi modules are equivalent to the equipment specified in section 1.4. This is due to the protection and mine resistance of the ambulances that must be preserved when the combi modules are mounted inside the vehicle.

**1.2. Description and definitions**

The requirement specification, cf. section 1.4, describes all the requirements for the acquisition and consists of six columns with the following information:

|  |  |
| --- | --- |
| "#" | ID number |
| "Requirement" | Requirement description |
| "Classification" | The classification of the requirement as further described in section 1.3 |
| "DALO remarks" | Further information regarding the requirement |
| "Requirement compliance" | The tenderer's indication of compliance (YES or NO) |
| "Tender description" | Requirements regarding the tenderer's compliance description |

**1.3. Classification**

All requirements are mandatory requirements (SHALL) and shall be fulfilled by the tenderer. If just one of the mandatory requirements is not fulfilled, the tenderer's tender will not be taken into further consideration.

**1.4. Requirement and response sheet**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **#** | **Requirement** | **Classification** | **DALO remarks** | **To be filled out be the tenderer** | | |
| **Requirement compliance**  **(tick a box)** | | **Tenderer's description** |
| **YES** | **NO** |
| 1 | The combi modules shall be Weinmann Combi MODULE (Part no. WM 22210-0006) | **SHALL** | DALO notes that it is imperative that the offered combi modules are equivalent to the equipment specified in section 1.4. This is due to the protection and mine resistance of the ambulances that must be preserved when the combi modules are mounted inside the vehicle. |  |  |  |
| 2 | The vendor must supply 50 pcs. | **SHALL** |  |  |  |  |
| 3 | The delivery time must be less than 80 calendar days from submission of the purchase order. | **SHALL** |  |  |  |  |