**Requirement Specification Viking Pro Drysuits**

1. **Requirements**

**1.1. Description of the requirement**

DALO wants to acquire 42 non-magnetic Viking Pro rubber drysuits for various types of divers. DALO notes, that it is imperative that the offered suits are of the type, configuration and sizes specified in section 1.4, as they will be used in conjunction with existing suits and other equipment.

**1.2. Description and definitions**

The requirement specification, cf. section 1.4, describes all the requirements for the acquisition and consists of six columns with the following information:

|  |  |
| --- | --- |
| "#" | ID number |
| "Requirement" | Requirement description |
| "Classification" | The classification of the requirement as further described in section 1.3 |
| "DALO remarks" | Further information regarding the requirement |
| "Requirement compliance" | The tenderer's indication of compliance (YES or NO) |
| "Tender description" | Requirements regarding the tenderer's compliance description |

**1.3. Classification**

All requirements are mandatory requirements (SHALL) and shall be fulfilled by the tenderer. If just one of the mandatory requirements is not fulfilled, the tenderer's tender will not be taken into further consideration.

**1.4. Requirement and response sheet**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **#** | **Requirement** | **Classification** | **DALO remarks** | **To be filled out be the tenderer** | | |
| **Requirement compliance**  **(tick a box)** | | **Tenderer's description** |
| **YES** | **NO** |
| **1** | The dry suit shall be a Viking Pro 1000 (Product identification code/Part number 2200010000) | SHALL |  |  |  |  |
| **2** | The configuration of the dry suit shall be as follows:  Certified according to  EN14225-2:2005 : Yes Standard : Yes Rear entry : Yes Nonmagnetic zipper : Yes HD : Yes Relief zipper : Yes Viking arm marking : Yes Military marking (all black/embosed) : Yes Nonmagnetic valves / hose : Yes Inlet valve placement : Left thigh Exhaust valve placement : Upper left arm (std) Inlet valve (NM) : Si-Tech Std nonmagnetic valve Exhaust valve (NM) : Si-Tech X2 nonmagnetic valve black lid Hose (NM) : NO Latex neckseal : Surveyor/Latex, Std Glued on suit : Yes Latex cuff : Pro cuff Rubber sole size : Standard | SHALL |  |  |  |  |
| **3** | The supplier shall supply 31 of size 03/Extra Large (XL) | SHALL |  |  |  |  |
| **4** | The supplier shall supply 11 of size 02/Large | SHALL |  |  |  |  |
| **5** | The delivery time must be less than 84 calendar days from submission of the purchase order. | SHALL |  |  |  |  |