**The Danish Defence Acquisition and Logistics Organization**

**Tender for Ruggedized Single Ear Headset**

|  |  |  |
| --- | --- | --- |
| **Question submitted** | **Answer** | **Date of answering** |
| *Question no. 1:*   * What is the purpose of the “dual PTT” requirement. Please elaborate ? | For Requirement specification no. 2:  The radio RF-7800S offers a dual PTT functionality to toggle between talk groups. This dual functionality is needed on the headset cable. | 29-07-2019 |
| *Question no. 2:*  What is the application of this product that would require the frequency range of 400Hz – 18kHz. Please elaborate why 18 kHz is required, since this is unusual and up to approx.15 kHz is typically more than sufficient ? Also the lower frequency range is fairly unique, so please confirm if frequencies below 400 Hz is acceptable or why this is not the case ? | For Requirement specification no. 7:  Looking once more at the specifications of our existing different headset in use, we will accept a reduction to this requirement no.7:  Minimum Frequency Range 400Hz to 10kHz. | 29-07-2019 |
| * *Question no. 3* * In tender conditions the following is stated: *“Time of delivery 30 % - Please note no. 8 at Requirement Specification.”* Assume this is a mistake and reference should be to no.13 ? | Concerning Tender condition.no. 4:  And this is of course correct,  The correct text should be:  *“Time of delivery 30 % - Please note no. 13 at Requirement Specification.”* | 29-07-2019 |
| * *Question no. 4* * Pricing is required for 1.700 units. 200 delivered within max 10 weeks and remaining 1.500 units with max. 150 days delivery time). Will purchase be in minor batches over the 3 year period or will purchase be in one order/batch ? | Tender conditions no. 7:  One Purchase Order will be given for 1700 units and delivery will be split into 3 or 4 batches during a 3 year period. | 29-07-2019 |
| *- Question no. 5*  Under bullet point 7 in Tender Conditions it is stated that tender shall only contain the following: 1*) Cover letter – preferably using the DALO template 2) Filled out Requirement Specification.* Assume a datasheet should be included in the response, as mentioned in specifications point 10 ? | Concerning Tender conditions 7.  Once again you assume correct.  Datasheet must be included  In your tender. | 29-07-2019 |