**The Danish Defence Acquisition and Logistics Organization**

**Tender for Textile Boot Bags**

|  |  |  |
| --- | --- | --- |
| **Question submitted** | **Answer** | **Date of answering** |
| *Question no. 1:*Regarding Appendix 1 (TT35201), snit A-AIs it correct that the drawings in Appendix 1, snit A-A is seen from the side of the bag and shows that there are 2 folds? One in 10 mm and one in 25 mm? | *Answer no. 1:* Yes that is correct. | 03.06.2020 |
| *Question no. 2:*Regarding Appendix 1 (TT35201), snit B-BIs it correct that drawings in Appendix 1, snit B-B is seen from above and shows one fold of 10 mm? | *Answer no. 2:* Yes that is correct. | 03.06.2020 |
| *Question no. 3:*Will DALO be able to send a picture of the fabric material for the Textile Boot Bags?For example, an image of the material the fabric should be made of (I have your specifications in the material). | *Answer no. 3:*See the attached:* *Boot\_Bag\_1.jpg*
* *Boot\_Bag\_2.jpg*
 | 03.06.2020 |
| *Question no. 4:*Is the Textile Boot Bags a product DALO have today? | *Answer no. 4:*Yes. | 03.06.2020 |
| *Question no. 5:*Can 330Dtex be accepted in the production of the Textile Boot Bags? | *Answer no. 5:*No. 330 Dtex is not equivalent to 250 – 300Dtex and DALO cannot change the mandatory requirement.  | 03.06.2020 |